\*

The Technical Reference Manual for the Full-Spatial Median-Free-Liquid Photonic bit(s) Transfer Module 276,480-bit analog/digital Computer Processor Architecture.

\*

Draft number 1

Drafted by Dr. Thomas Catalano

<tomcatalano@outlook.com>

\*

\*

\*

Overview:

This working draft will outline the full-spatial 276,480-bit computer processor architecture with the newly

designed median-free-liquid via photonic bit transfer module processor computer system from

design, engineering and programming.

\*

\*

\*

Diversity in technology:

As we continued into the 21st century yearning for seamless interconnectivity and

quasi-operational machines new designs were needed. One such designed utility was invented

and engineered by Dr. Thomas Catalano in AD 2014, the Full-Spatial median-free-liquid

photonic bit(s) transfer module 276,480-bit analog/digital computational processor/computer so to the design,

engineering and guidelines to coherently run arbitrary instruction sets to the architecture and

system.

\*

\*

\*

Designing the utility:

The core photonic processing unit runs two opposing single(main plate) and/or overlayed(grid plate system added to the main plate for true parallelism multi-processing) lenses for data stream(s) as RGB color spectrum

number sequencing as one "channeled" beam rays streaming like a thread in a "silica" based microprocessor. The

"channeled" stream is sequencing data numerically by referencing the RGB color spectrum.

A single standalone complete center-cycling semiconductor at the central switching/processing module hubed to the I/O lenses on each side of the

"U-shaped" unit embedding the (2)276,480-pin injection on each side then connecting to the semiconductors centralized connector system.

\*

\*

\*

Engineering programming:

The how, what and where of it.

/

How do we now handle/define units of bit(s)-to-precession float number counts as hardware

architecture is not limited to bit transfer unit.

/

We need new and add to current structured binary translations to define spunit as per

independent of 360\_degree area cavity trace route.

/

No matter the size of cavity, defining measurable rate is compared by data rate (d rate) to

"defined" transmitting median(tm rate).

/

############The "spectra unit" ############

/

-requires unit of measurement for RGB color/spectrum(by)data stream coverage to

compute rate() per time/frame at actual area computing

-A required unit of measurement for one(1) "spectra unit" as per a "IEEE Std" would define the

scale to calculate 0-100% cofactor of continuous bit transfer rate..

-()3×256=768×360=(276,480-bit spectral cavity processor); spectra by one(n area) cavity or

multi(n area) per cavities spectrums total area of calculating/actual area used =

-now we have one "276,480-bit "spectra(s)"" in (n) area;

data at()

×

per second of ON time=(n)

/

\*

\*

\*

Programming:

We will contextualize current programming languages to building a stand alone language.

/

Arithmetic…

IE. Floating point numbers...

/

=

([(Floating-Point\*/0×

Floating-Point\*/0)])

=

((3×256)[x\*])(k\*))]

/

new programming language/packaging required for pragmatic system requirements needed for

operations/conversions to...

Now;

-we fill in with architecture hardware specifications..

/

[]

[]

[]

[]

[]

[]

[]

[]

[]

/

All (spectral areas(undetermined defined range) by(×)×(the cavity(x)) are deterministic[x] and

accountable (per unit(xOFn)) of(per unit filled(xOFn)=(spectral range(3×256)×(n))...

/

Defined area of spectral area as standard;

-material per unit sq. ?...

/

then-

/

-we know we can not use the ranges defined by present standards or programming languages

required to define the future approved ranges of grouped numbers then to be translated into

current silica microprocessor architecture.

/

/

Example- progmatic inference;

/

"bit" lang for the Full-Spatial Quantum Computer);

-Due to new architecture non-restrictions setting implicit charters are required…

1. Looped verification of spectral timed events

2. Bounds vs. Latency = ~0~

3. Numbered/naming power of (n) number sequensing in blocks named(x)

/

!Level of standard!...machine always ON or always OFF…

...okay let's GO!

/

Example-

/

Formatting/Transfer from the "bit" lang programming language to…

-Registry requirements per area of available spectral cohesion rate..

-library's to systemically w/ Floating-Point

File format and/or runing sums to target architecture whether dependent to specific output of the

Full-Spatial computer processor(ie. operating system specific to the FSCP).

/

\*

\*

\*

-on continuing this working draft the emphasis will be maximum hardware output with a stand

alone standardized operating/programming system/language to utilize structured semantics in info-packaging the new 276,480-bit computer processor architecture.

//

Draft number 1.

\*